|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 貨號 | 英文/中文品名 | 簡述 | 圖片 | 原文敘述 | 網址 |
| VK-10201 | Test block (transparent)  透明測試塊 | 用於聲波實驗使用 |  | · Dimensions: 150 mm × 80 mm × 40 mm  · Material: acrylic, transparent  · Sound velocity: ≈ 2700 m/s (longitudinal) | <http://www.gampt.de/content/cms/front_content.php?idcat=82&idart=149> |
| VK-10204 | Test block (black)  黑色測試塊 | 用於聲波實驗使用 |  | · Dimensions: 150 mm × 80 mm × 40 mm  · Material: acrylic, black (opaque)  · Sound velocity: ≈ 2700 m/s (longitudinal)  · Density: 1.2 g/cm³  · Defects: 11 | <http://www.gampt.de/content/cms/front_content.php?idcat=82&idart=149> |
| VK-  10233 | Delay line for angle 17°  延遲線楔17° | 用於調整角度 |  | · Material: acrylic  · Sound velocity in acrylic: ≈ 2700 (longitudinal)  · Angle of incidence (delay line): 17° | <http://www.gampt.de/content/cms/front_content.php?idart=162> |
| VK-  10234 | Delay line for angle 38°  延遲線楔38° | 用於調整角度 |  | · Material: acrylic  · Sound velocity in acrylic: ≈ 2700 (longitudinal)  · Angle of incidence (delay line): 38° | <http://www.gampt.de/content/cms/front_content.php?idart=162> |
| VK-10235 | Delay line for angle 56°  延遲線楔56° | 用於調整角度 |  | · Material: acrylic  · Sound velocity in acrylic: ≈ 2700 (longitudinal)  · Angle of incidence (delay line): 56° | <http://www.gampt.de/content/cms/front_content.php?idart=162> |
| VK-10237 | Transceiver delay line (TOFD)  收發器延遲線楔 | 用於搭配探針，使用TOFD方法，測試不連續性 |  | A special probe is used in the testing for discontinuities with the TOFD method (time of flight diffraction). | <http://www.gampt.de/content/cms/front_content.php?idcat=82&idart=370> |
| VK-10240 | Test block for angle beam probe  測試塊(調整探針角度) | 用於調整探針角度 |  | The aluminium test block is for the adjustment of angle beam probes, regarding the refraction angle, sound velocity, sound emergence point and the length of the delay line. | <http://www.gampt.de/content/cms/front_content.php?idcat=82&idart=165> |
| VK-10241 | Crack depth test block  裂縫深度測試塊 | 用於進行不同深度量測 |  | The test block contains cracks with different depths. Using two different measuring techniques the cracks can be localised and their depths determined. | <http://www.gampt.de/content/cms/front_content.php?idcat=82&idart=166> |
| VK-10242 | Discontinuity test block  不連續性測試塊 | 用於測試不連續性的試塊 |  | The aluminium test block contains different reflector types that can be used for producing echoes. | <http://www.gampt.de/content/cms/front_content.php?idcat=82&idart=167> |
| VK-20230 | Projection lens  投射鏡 | 用於投射聲光效應的聲波 |  | The plano-convex optical lens is placed, for the projection of standing ultrasonic waves, in the beam path between laser source and ultrasonic wave, to produce a divergent laser beam. | <http://www.gampt.de/content/cms/front_content.php?idcat=84&idart=194> |
| VK-19004 | Advanced applications of ultrasound  超聲波進階應用實驗組(超聲波的剪切波與表面波) | | | | |
| VK-10400 | Ultrasonic echoscope GS200  超聲波回聲測深儀 | 連接探針後，用於進行聲波實驗探索 |  | The GS200 is a high-resolution ultrasonic measurement system for connection to a PC or an oscilloscope. | <http://www.gampt.de/content/cms/front_content.php?idcat=82&idart=429> |
| VK-10151 | Ultrasonic probes 1 MHz  超聲波探針1MHz | 超聲波探針1MHz |  | The blue-marked ultrasonic probes are characterised by high sound intensity and short sound impulses. | <http://www.gampt.de/content/cms/front_content.php?idart=153> |
| VK-10152 | Ultrasonic probes 2 MHz  (GS200)  超聲波探針2MHz | 超聲波探針2MHz |  | With a frequency of 2 MHz, these red-marked probes are suitable for a wide range of applications. | <http://www.gampt.de/content/cms/front_content.php?idart=153> |
| VK-10154 | Ultrasonic probes 4 MHz  (GS200)  超聲波探針4MHz | 超聲波探針4MHz |  | The 4 MHz probes (green-marked) are characterised by extremely short dying out behaviour and thus the highest axial resolution power. | <http://www.gampt.de/content/cms/front_content.php?idcat=82&idart=153> |
| VK-10218 | Shear wave set  剪波套件 | 用於進行縱向波至剪波的相關實驗 |  | Shear waves have a sound velocity that differs from the longitudinal wave. With this experiment equipment, the angle-dependent transition from longitudinal to shear waves can be measured. | <http://www.gampt.de/content/cms/front_content.php?idcat=82&idart=154> |
| VK-10231 | Rayleigh wave attachment pair  雷里波元件 | 用於刺激和接收在樣品中的表面波 |  | With this attachment adjusted to aluminium, surface waves (Rayleigh waves) can be stimulated and received in a sample. | <http://www.gampt.de/content/cms/front_content.php?idcat=82&idart=160> |
| VK-10232 | Rayleigh wave test block  雷里坡測試塊 | 用於表面波實驗 |  | The material sample for investigation with Rayleigh waves has an intact surface side, at which the velocity of Rayleigh waves can be determined in transmission mode. | <http://www.gampt.de/content/cms/front_content.php?idcat=82&idart=161> |
| VK-10300 | Lamb wave set  藍姆波套件 | 進行藍姆波相關實驗 |  | With the set the frequency-dependent propagation velocity (dispersion) of ultrasonic waves in a thin glass plate (Lamb waves) can be measured. | <http://www.gampt.de/content/cms/front_content.php?idcat=82&idart=374> |
| VK-70200 | Ultrasonic gel(250ml)  超聲波凝膠 | 用於超聲波實驗使用 |  | A coupling medium must be used for the coupling of the ultrasonic probes to the test object. | <http://www.gampt.de/content/cms/front_content.php?idcat=82&idart=169> |
| VK-10450 | Hydrophone for GS200  水聽器 | 測量聲場特性 |  | The hydrophone can be used to measure the characteristics of sound field of an ultrasonic probe | <http://www.gampt.de/content/cms/front_content.php?idart=168> |
| VK-19008 | Acousto-optical effects  聲光轉換實驗組 | | | | |
| VK-20100 | cw generator SC600  連續波產生器SC600 | 可連接超聲波探針產生超聲波以及連接雷射元件控制電壓輸出，並且擁有訊號產生器的功能，可靈活的進行多種實驗 |  | The cw generator SC600 permits the generation of continuous sound waves (continuous wave - cw) with high power over a wide frequency range up to 20 MHz. | <http://www.gampt.de/content/cms/front_content.php?idart=176> |
| VK-20200 | Debye-Sears set  德拜-西爾斯套件 | 用於德拜-西爾斯實驗以及超聲波在樣品池投影 |  | The generation of standing waves for the Debye-Sears experiment and the projection of ultrasonic waves in a special sample reservoir, with the probe adjustment of which the ultrasonic probe can be aligned so that incidence is precisely perpendicular. | <http://www.gampt.de/content/cms/front_content.php?idart=188> |
| VK-20303 | Photodiode receiver  光電二極體接收器 | 使用內建放大器的光電二極體接收器，可定量記錄雷射強度。 |  | With this photodiode receiver with built-in amplifier, a quantitative recording of the intensity of the laser light is possible. | <http://www.gampt.de/content/cms/front_content.php?idart=400> |
| VK-20302 | Adjustable reflector  可調整反射器 | 反射器透過三點調整固定在支架上。可進行水平或垂直使雷射對準目標物 |  | It can be horizontally and vertically adjusted to align the laser beam precisely to the target object. | <http://www.gampt.de/content/cms/front_content.php?idart=399> |
| VK-20301 | Beam splitter  分束器 | 半透射反射器被用於雷射的分束器 |  | A semipermeable reflector is used as a beam splitter for laser light. The transmission/reflection ratio is 1:1 | <http://www.gampt.de/content/cms/front_content.php?idart=398> |
| VK-20227 | Acoustic absorber  吸音器 | 用於防止在AOM實驗不需要的聲音反射或是使用於熱聲感應器 |  | The acoustic absorber consists of a special silicone material that is able to absorb ultrasonic waves almost completely. | <http://www.gampt.de/content/cms/front_content.php?idart=208> |